Part 1:

How can you verify that both passwords were configured correctly? Answer:

After exit EXEC mode, the switch will propmt you for password and will prompt you second time when accessing the priveleged EXEC mode.

Which command do you issue to accomplish this step? Answer: exit, copy run start

Part 2:

Were you successful? Explain. Answer: Unsuccessful, because the switches haven’t been configured with IP address.

Part 3:

Why would we configure it with IP address? Answer: In order for you to connect remotely to switch, you need to assing it IP address. The defauly configuration on switch is to have the management of switch controlled through VLAN 1.

Why do you enter no shutdown command? Answer: The no shutdown command administratively places the interface in active state.

Which command is used to save the configuration file in RAM to NVRAM? Copy running-config startup-config