Part 1:

What is the setting for bits per second? Answer: 9600

What is the prompt displayed on the screen?: Answer: S1

1. Which command begins with the letter ‘C’? Answer: Connect
2. Which commands are displayed? Answer: telnet, terminal, traceroute
3. Which commands are displayed? Answer: telnet terminal

Part 2:

1. What information is displayed for the enable command? Answer: turn on to privileged commands
2. What displays after pressing the Tab key? Answer: Enable

What would happen if you typed te at the prompt? Answer: Nothing

1. How does the prompt change? Answer: S1#
2. How many commands are displayed now that privileged EXEC mode is active? Answer: clear, clock, configure, connect, copy
3. What is the message that is displayed? Answer: configuring from terminal, memory, or network[terminal]?
4. How does the prompt change? Answer: S1(config)#

Part 3:

1. What information is displayed? Answer: \*0:13:14.50 UTC Mon Mar 1 1993
2. What information is displayed? Answer: % Incomplete command
3. What information is displayed? Answer: set, Set the time and date
4. What information is being requested? Answer: hh:mm:ss Current Time

a)

b) S1# cl<tab> Questions: What information was returned? Answer: Nothing

S1# clock Question: What information was returned? Answer: % Incomplete command

S1# clock set 25:00:00 Question: What information was returned? Answer: Invalid input detected at “^” marker

S1# clock set 15:00:00 32 Question: What information was returned? Answer: Invalid input detected at “^” marker